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Large Pull-Out Pivot Wall Mount for 55" to 75" TVs - HPF675
SECTION 27 05 29.13
HANGERS AND SUPPORTS FOR A-V EQUIPMENT
GENERAL
SUMMARY
Section includes furnishing and installation of large pull-out pivot wall mount system designed to support flat-panel audio-visual displays ranging from 55 to 75 inches in hospitality, residential, commercial, institutional, and professional environments.
Mounting system shall be Peerless-AV® Large Pull-Out Pivot Wall Mount, Model HPF675, or approved equal meeting all specified performance, swivel adjustment, pull-out access, compatibility, security, installation, and serviceability requirements without modification to the mounting system or accessories.
Includes wall mount assembly, universal adaptor brackets, mounting hardware, security hardware, cable management accessories, and manufacturer-approved accessories required for a complete installation.
Coordinate mounting locations with wall backing, recessed electrical boxes, low-voltage pathways, cable routing, and wall finishes to ensure proper installation, pull-out access, and viewing clearances.
RELATED SECTIONS
Division 06 - Wood: Blocking and backing within wall assemblies.
Division 09 - Finishes: Wall finishes, surface preparation, and non-load-bearing metal framing at mounting locations.
Division 26 - Electrical: Coordination of power supply, conduit, junction boxes, recessed outlet boxes, and data connections associated with wall-mounted displays.
Division 27 - Communications: Low-voltage cabling and cable routing associated with display installation.
REFERENCES
UL 2442 - Flat Panel Display Mounting Devices.
ADA Standards for Accessible Design, where applicable.
NFPA 70 - National Electrical Code (NEC).
ASTM C-90 - Standard Specification for Load-Bearing Concrete Masonry Units (applicable where concrete masonry unit (CMU) substrates are used).
AISI S100 - North American Specification for the Design of Cold-Formed Steel Structural Members.
AISI S211 - North American Standard for Cold-Formed Steel Framing.
Manufacturer’s published installation instructions and standard installation procedures.
Applicable local building codes and regulations governing mounting systems and accessibility.
SUBMITTALS
Product Data Sheets: Manufacturer’s current technical literature indicating dimensions, materials, finishes, load ratings, swivel ranges, pull-out extension distances, mounting patterns, and compliance listings.
Shop Drawings: Indicating mounting locations, pull-out clearances, viewing angles, and coordination with electrical and low-voltage systems.
Installation Instructions: Manufacturer’s current installation instructions and recommended anchorage methods.
Warranty Documentation: Manufacturer’s standard warranty information.
Accessory Data: Technical data for optional or specified accessories, if applicable.
QUALITY ASSURANCE
Manufacturer shall have a minimum of ten (10) years experience producing commercial A-V mounting systems of similar type, size, and complexity.
Products shall be UL listed and labeled by a nationally recognized testing laboratory and shall comply with applicable safety and performance standards.
Installer shall be experienced in installation of commercial AV mounting systems of similar size, weight and articulation complexity.
DELIVERY, STORAGE, AND HANDLING
Deliver products in original factory packaging with labels intact.
Store products indoors in a clean, dry location, protected from moisture, physical damage, and exposure to construction activities.
Protect from damage due to weather, moisture, construction operations and excessive temperature
This product is intended for indoor use only. Use outdoors may lead to product failure or personal injury.
[bookmark: _GoBack]WARRANTY
Provide manufacturer’s limited 5 year warranty covering defects in materials and workmanship under normal use and service conditions.
PRODUCTS
MANUFACTURERS
Basis-of-Design Product:
Peerless-AV® Large Pull-Out Pivot Wall Mount
Model: HPF675
Display Compatibility: 55” to 75” TVs
Manufactured by Peerless-AV®, 2300 White Oak Circle, Aurora, IL 60502; Phone (800) 865-2112, (630) 375-5100
Website: www.peerless-av.com
Substitutions:
Approved equal products shall meet or exceed all specified VESA compatibility, load capacities, pull-out extension capabilities, swivel ranges, locking functionality, auto-centering feature, mounting compatibility, installation methods, maintenance accessibility, and UL listing requirements without requiring redesign of wall conditions, structural reinforcement, or modification to accessories or mounting components, in accordance with Section 01 25 00.
PERFORMANCE REQUIREMENTS
Listings:
UL Listed and labeled in compliance with UL 2442 - Flat Panel Display Mounting Devices.
Comply with applicable environmental and material compliance requirements, including RoHS and TAA compliance. 
Acceptable Wall Substrates: 
Wood studs: Minimum 2” x 4” nominal size. Designed for dual 16 inches on center stud.
Steel studs: Dual 16 inches on center stud configuration.
Solid concrete: Minimum 8” thick with a minimum compressive strength of 2,000 psi.
Concrete masonry unit (CMU): Must meet ASTM C-90 specifications with a minimum nominal width of 8”. Do not drill into mortar joints.
Load Capacity:
Mounting system shall support displays weighing up to 80 lb (36 kg) without permanent deformation or loss of structural integrity.
Display Size Range:
Compatible with flat panel displays ranging from 55 inches to 75 inches or larger, subject to display weight and VESA mounting pattern compatibility.
Mounting Pattern Compatibility:
Compatible with VESA® mounting patterns ranging from 200 x 200 mm to 400 x 400 mm. 
Pull-Out and Swivel Functionality
Mounting system shall provide pull-out pivot functionality allowing service access behind display assemblies. 
Mounting system shall provide swivel adjustment capability for flexible viewing angle positioning.
55-inch displays: Up to ±30 degrees swivel. 
75-inch displays: Up to ±22 degrees swivel. 
Mounting system shall maintain centered display positioning during extension and retraction movement. 
Fully retracted mount depth shall be approximately 2.83 inches (72 mm). 
Fully extended mount depth shall be approximately 12.95 inches (329 mm). 
Installation Features:
Mounting system shall incorporate pull-out pivot arm design providing simplified maintenance access behind display assemblies.
Provide locking feature allowing mounted display to be secured against wall surface to minimize tampering and unauthorized movement.
I-shaped adaptor plate configuration shall minimize obstruction of display power, signal, and connection locations.
Design shall provide smooth extension and retraction movement while maintaining structural stability throughout swivel range.
PRODUCT SPECIFICATIONS
Physical Dimensions:
Overall Dimensions (W x H x D): 25.25” x 16.75” x 2.83”-12.95” (641 x 425 x 72-329 mm)
Product Weight: 17.60 lb (8 kg)
Load Capacity: 80 lb (36 kg)
Swivel Range: ±30° for 55” displays | ±22° for 75” displays
Min VESA Pattern: 200 x 200 mm
Max VESA Pattern: 400 x 400 mm (15.75” x 15.75”)
Depth (retracted/extended): 2.83”-12.95” (72-329 mm)
Unique Feature: Locking rod mechanism
Finish: Powder Coat, Black
Warranty: Limited 5 Year Warranty
Package Specifications:
Package Dimensions (W x H x D): 28.00” x 10.63” x 4.00” (711 x 270 x 102 mm)
Package Ship Weight: 21.20 lb (10 kg)
Package UPC: 735029349808
Package Contents: Wall mount, Universal Adaptor, wall and display installation hardware, installation instructions
Included Hardware:
Includes manufacturer-provided wall and display mounting hardware required for complete installation.
MATERIALS AND FINISH
Structural components shall be fabricated from heavy-duty steel suitable for supporting specified loads.
Finish shall be manufacturer’s standard powder coat finish.
Color: Black.
ACCESSORIES
Provide manufacturer-approved accessories compatible with the mounting system and installation requirements.
Accessories shall not reduce rated load capacity or interfere with mounting system performance.
EXECUTION
EXAMINATION
Verify wall construction, substrate type, and load-bearing capacity are suitable for installation of the pull-out pivot wall mount system and supported display loads.
Verify mounting locations, pull-out clearances, swivel movement range, and coordination with electrical and low-voltage systems prior to installation.
For wood stud walls: use a stud finder to locate and mark stud center lines. Confirm studs are a minimum of 2” x 4” nominal size and that gypsum board does not exceed 5/8” in thickness.
For metal stud walls: verify metal stud framing complies with AISI S100 or AISI S211 requirements and minimum gypsum board thickness requirements specified by manufacturer.
For concrete walls: confirm wall is at least 8” thick with a minimum compressive strength of 2,000 psi.
For concrete masonry unit (CMU) walls: confirm blocks meet ASTM C-90 specifications and have a minimum nominal width of 8”. Identify mortar joint locations to be avoided. 
INSTALLATION
Install mounting system in accordance with manufacturer’s written instructions and applicable codes.
Secure mounting system to structural framing or approved substrates using manufacturer-recommended fasteners and anchorage methods.
Coordinate mounting locations with wall blocking, electrical rough-in, recessed outlet boxes, and cable routing systems.
Verify mounting location provides adequate structural support for articulated loads generated during pull-out and swivel operation.
Verify adequate clearance for full extension and swivel operation prior to final installation.
Adjust mounting system for final level, alignment, extension range, and viewing orientation after installation.
Verify completed installation is secure, properly aligned, and fully operational prior to final acceptance.
CLEANING AND PROTECTION
Remove debris, packaging materials, and installation residue from project site.
Verify pull-out pivot and swivel operate freely without obstruction after cleanup.
Protect installed equipment from damage until substantial completion and final acceptance.
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