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Universal Ultra-Slim Scissor Wall Mount
SECTION 27 05 29.13
HANGERS AND SUPPORTS FOR A-V EQUIPMENT
GENERAL
SUMMARY
This section includes furnishing and installation of extendable flat panel wall mount systems designed for supporting large-format audio-visual displays in commercial, institutional, and professional environments.
Mounting system shall be Peerless-AV’s SmartMount® Universal Ultra-Slim Scissor Wall Mount (STS680) or an approved equal meeting all performance, adjustment, compliance, compatibility, and installation requirements specified herein, without modification to the mounting system or accessories.
Includes all hardware, brackets, fasteners, and accessories required for a complete installation.
Coordinate mounting system depth, service access, and attachment locations with recessed electrical boxes, low-voltage outlets, and in-wall components to ensure proper fit and accessibility.
[bookmark: _GoBack]RELATED SECTIONS
Division 06 - Wood: Backing, if mounting to wood substrates.
Division 09 - Finishes: Wall finishes, surface preparation, and non-load-bearing metal framing at mounting locations.
Division 26 - Electrical: Coordination of power supply, conduit, junction boxes, and data connections associated with wall-mounted displays.
REFERENCES
UL 2442 - Flat Panel Display Mounting Devices.
ADA Standards for Accessible Design.
Manufacturer standard installation procedures.
NFPA 70-2023, National Electrical Code (NEC).
Applicable local building codes and regulations governing mounting systems and accessibility.
SUBMITTALS
Product Data Sheets: Manufacturer’s technical literature indicating materials, dimensions, load ratings, adjustment ranges, mounting patterns, and compliance listings.
Shop Drawings: Showing mounting locations and clearances.
Installation Instructions: Manufacturer’s current installation instructions and recommended anchorage details.
Warranty Documentation: Manufacturer’s standard warranty information.
Accessory Data: Technical data for optional or specified accessories, if applicable.
QUALITY ASSURANCE
Manufacturer shall have a minimum of ten (10) years experience producing commercial A-V mounting systems of similar type, size, and complexity.
Products shall be listed and labelled by a nationally recognized testing laboratory and shall comply with applicable safety and performance standards.
Installer shall be experienced in installation of commercial AV mounting systems of similar size and complexity.
DELIVERY, STORAGE, AND HANDLING
Deliver products in original factory packaging with labels intact.
Store products indoors in a clean, dry location, protected from moisture, physical damage, and exposure to construction activities.
Protect from damage due to weather, moisture, construction operations and excessive temperature
WARRANTY
Provide manufacturer’s lifetime warranty covering defects in materials and workmanship under normal use and service conditions.
PRODUCTS
MANUFACTURERS
Basis-of-Design Product:
Peerless-AV SmartMount® Universal Ultra-Slim Scissor Wall Mount
Model STS680, STS680-1UCM3 or STS680-2UCM3 
Manufactured by Peerless-AV, 2300 White Oak Circle, Aurora, IL 60502; Phone (800) 865-2112, (630) 375-5100
Website: www.peerless-av.com
Substitutions:
Approved equal products shall meet or exceed all specified load capacities, adjustment ranges, ADA compliance, UL listing, accessory compatibility, and installation requirements without requiring redesign of wall conditions or structural reinforcement, in accordance with Section 01 25 00.
PERFORMANCE REQUIREMENTS
Listings:
Mounting system shall be UL 2442 Listed for installation on wood studs, metal studs, concrete, or masonry substrates and bear the UL Listing Mark.
Acceptable Wall Substrates: 
Steel studs, wood studs, concrete, and cinder block when installed per manufacturer’s instructions.
Load Capacity:
Mounting system shall support a minimum static load of 250 lb (113.4 kg) without permanent deformation or loss of structural integrity.
Display Size Range:
Compatible with flat panel displays ranging from 49 inches to 120 inches or larger, subject to display weight and VESA mounting pattern compatibility.
Mounting Pattern Compatibility:
Support VESA mounting patterns ranging from 200 × 100 mm to 1000 × 600 mm
Depth Adjustment:
Mount shall incorporate an extendable scissor-arm design to allow forward service access of a minimum of 12.8” (325mm)  and allow maintenance and connection access without removal of the display from the mount
Provide adjustable and lockable depth positions ranging from 1.8 inches to 7.8 inches (46-198 mm), adjustable in the field, marked with high visibility silkscreen for easy identification
ADA Compliance:
When installed in accordance with manufacturer instructions and used with displays not exceeding 2.2 inches (56mm) in depth, the complete installed assembly shall comply with ADA protrusion limits, achieving a total projection of 4 inches or less without removal of accessories or components.
Adjustment Capabilities:
Post-installation leveling: 1” (25mm) of total adjustment or ± ½” (12mm), marked with high visibility silkscreen for easy identification
Plumb adjustment: Minimum of 2 degrees to accommodate wall irregularities, marked with high visibility silkscreen for easy identification
Tilt:
Provide optional IncreLokTM feature offers fixed, lockable tilt positions adjustable from 0 degrees to 15 degrees in 2.5° increments, marked with high visibility silkscreen for easy identification
Lateral Shift:
Mount shall provide lateral shift capability to allow horizontal positioning of the display after installation.
MATERIALS AND FINISH
Structural components shall be fabricated from heavy-duty steel suitable for supporting specified loads.
Finish: Manufacturer’s standard scratch-resistant fused epoxy coating, black.
SEISMIC QUALIFICATION
Seismic qualification shall be demonstrated by one of the following methods, as acceptable to the AHJ:
Shake-table testing in accordance with ICC-ES AC156 for the specific product, model, and configuration.
Seismic qualification by analysis in accordance with ASCE/SEI 7, prepared and sealed by a Professional Engineer licensed in the project jurisdiction.
Manufacturer certification indicating compliance with seismic requirements, supported by test data or sealed engineering.
Seismic qualification documentation shall be specific to the installed configuration, including:
Product model numbers and accessories.
Maximum allowable equipment weights and eccentric loading limitations.
Anchorage type, size, and substrate assumptions.
Orientation and mounting conditions.

ACCESSORIES
Provide manufacturer-designed modular accessories compatible with the mounting system, including camera mounts, UC mounting plates, power management brackets, cable management components, and component mounting plates, as required for the installation.
Accessories shall be manufacturer-approved and shall not reduce the rated load capacity or interfere with the performance or compliance of the mounting system.
Accessories shall be manufacturer-designed components specifically engineered for compatibility with the Basis-of-Design mounting system. Third-party accessories requiring field modification shall not be permitted.
ACC-UCM3 - Universal Component Mounting Bracket with toolless installation, 10lb (4.5kg) weight capacity. Universal AV Component Mount (ACC-UCM3) allows AV components to be installed inside or outside of the wall plate.
ACC-STSVCB – Universal Video Conferencing Bar / Sound Bar mounting bracket with toolless height adjustment, 15 lb (6.8kg) weight capacity and ability to mount above or below the display
ACC-STSPTZ – Universal Pan/Tilt/Zoom (PTZ) Camera mounting bracket with toolless height adjustment, 15 lb weight capacity and ability to mount above or below the display
ACC-STSPDU – Low profile PDU mounting bracket for SurgeX DisplayPak+ power distribution units (SX-DPP-102 and SX-DPP-104), 10 lb (4.5kg) weight capacity
ACC-STSCF1 – Low profile mounting bracket for Crestron Flex 260/200 UC Engine,10 lb (4.5kg) weight capacity 
ACC-STSCF2 – Low profile mounting bracket for Crestron Collab Compute, 12 lb (5.4kg) weight capacity
ACC-STSLB – Cable Management Lacing Bracket, 15 lb (6.8kg) weight capacity
IB14X14-W – 14x14” in-wall box for recessed power and AV components, 25 lb (11.3 kg) weight capacity
IB14X9-W – 14x9” in-wall box for recessed power and AV components, 25 lb (11.3 kg) weight capacity
ACC615 – Peerless-AV metal stud fastener kit (6-pack)
EXECUTION
EXAMINATION
Verify wall construction, substrate type, and load-bearing capacity are suitable for installation of the mounting system.
Verify mounting locations, clearances, and coordination with power and data connections prior to installation.
INSTALLATION
Install wall mount system in strict accordance with manufacturer’s written instructions and applicable codes.
Installer shall verify stud gauge, spacing, and substrate conditions prior to installation. Notify Architect in writing if wall construction does not meet manufacturer’s minimum installation requirements. Do not proceed until discrepancies are resolved.
Secure mount to structural framing or approved substrates using manufacturer-recommended fasteners and methods.
Adjust mount to final alignment, including level, plumb, tilt, and depth, to achieve proper positioning of the display.
Verify completed installation is secure, properly aligned, and adjusted in accordance with specified performance requirements prior to final acceptance.
CLEANING AND PROTECTION
Remove debris, packaging materials, and construction residue from the installation area.
Protect installed equipment from damage until project completion and final acceptance.
END OF SECTION
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